INSTRUCTION MANUAL
Original instructions for
SALAD SPINNER

SD75SF
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[bookmark: _Hlk63155923]Keep these instructions with the appliance. 
You should read this user manual carefully before using the appliance.
[bookmark: _Hlk63171749]Dear Customer,
Thank you for purchasing this appliance. Please take a few minutes before starting operation of the appliance and read the following operating instructions.

1. Intended use 
1.1 This machine is designed for vegetable drying in restaurants, canteens and similar catering establishments. 
1.2 The machine is not intended to process for meet, fruit, fish. Otherwise, it might lead to damage of the machine, property or personal injury.
1.3 The machine is intended for commercial and indoor use by trained and skilled personnel familiar with these instructions.

The assortment is made up of one size: SD75SF
The machine body is built in stainless steel and for easy cleaning and maintenance. It has safety features compliant with the applicable safety Directives.

2. Safety regulations  [image: ]
2.1 Safety regulations
2.1.1 This appliance is intended for commercial use only and must not be used for household use.
2.1.2 The appliance must only be used for the purpose for which it was intended and designed. The manufacturer is not liable for any damage caused by incorrect operation and improper use.
2.1.3 Keep the appliance and electrical plug away from water and any other liquids. In the event that the appliance should fall into water, immediately remove plug from the socket and do not use until the appliance has been checked by a certified technician. Failure to follow these instructions could cause a risk to lives.
2.1.4 Never attempt to open the casing of the appliance yourself.
2.1.5 Do not insert any objects in the casing of the appliance.
1.1.6 Do not touch the plug with wet or damp hands.
2.1.7 Danger of electric shock! Do not attempt to repair the appliance yourself. In case of malfunctions, repairs are to be conducted by qualified personnel only.
2.1.8 Never use a damaged appliance! Disconnect the appliance from the electrical outlet and contact the retailer if it is damaged.
2.1.9 Do not immerse the electrical parts of the appliance in water or other liquids.
Never hold the appliance under running water.
2.1.10 Regularly check the power plug and cord for any damage. If the power plug or power cord is damaged, it must be replaced by a service agent or similarly qualified persons in order to avoid danger or injury.
2.1.11 Make sure the cord does not come in contact with sharp or hot objects and keep it away from open fire. To pull the plug out of the socket, always pull on the plug and not on the cord.
2.1.12 Ensure that the cord (or extension cord) is positioned so that it will not cause a trip hazard.
2.1.13 Always keep an eye on the appliance when in use.
2.1.14 As long as the plug is in the socket the appliance is connected to the power source.
2.1.15 Turn off the appliance before pulling the plug out of the socket.
2.1.16 Never carry the appliance by the cord.
2.1.17 Do not use any extra devices that are not supplied along with the appliance.
2.1.18 Only connect the appliance to an electrical outlet with the voltage and frequency mentioned on the appliance label.
2.1.19 Connect the power plug to an easily accessible electrical outlet so that in case of
emergency the appliance can be unplugged immediately. To completely switch off the appliance pull the power plug out of the electrical outlet.
2.1.20 Always turn the appliance off before disconnecting the plug.
2.1.21 Never use accessories other than those recommended by the manufacturer. Failure to do so could pose a safety risk to the user and could damage the appliance. Only use original parts and accessories.
2.1.22 This appliance is not intended for use by persons (including children) with reduced physical, sensory or mental capabilities, or lack of experience and knowledge.
2.1.23 This appliance must not be used by children under any circumstances.
2.1.24 Keep the appliance and its cord out of reach of children.
2.1.25 Always disconnect the appliance from the mains if it is left unattended or is not in use, and before assembly, disassembly or cleaning.
2.1.26 Never leave the appliance unattended during use.

2.2 Special Safety Regulations
2.2.1 The appliance is intended for commercial and indoor use by trained and skilled personnel familiar with these instructions.
2.2.2 This machine is designed for food processing in restaurants, canteens and similar catering establishments.
2.2.3 Any other use might lead to damage to the appliance or personal injury.
2.2.4 Do not place the appliance on a heating object (gasoline, electric, charcoal cooker, etc.) Keep the appliance away from any hot surfaces and open flames. Always operate the appliance on a level, stable, clean, heat-resistant and dry surface.
2.2.5 Danger of injury! Care is needed when operating or cleaning.
2.2.6 Caution! Securely route the power cord if necessary, in order to prevent unintentional tripping over and falling.
2.2.7 Do not use the appliance before it is properly assembled.
2.2.8 This appliance is not intended to be operated by means of an external timer or separate remote-control system.
2.2.9 Never bypass any safety interlocks on the appliance.
2.2.10 WARNING: ALWAYS switch off the appliance and unplug from electrical power supply before cleaning, maintenance or storage.
2.2.11 WARNING: ALWAYS keep hands, long hair and clothing away from the moving parts.
2.2.12 WARNING: Take great care when handling the rotating parts. 
2.2.13 Allow at least 15cm spacing around the appliance for ventilation purpose during use.
2.2.14 Do not wash the appliance with water or waterjet. Washing with water can cause leakage and increase the risk of electric shock. No parts are dishwasher safe.
2.2.15 Do not move the appliance while it is under operation. Unplug the appliance when moving and hold it at the bottom.
2.2.16 Special care should be taken when moving or transporting the appliance due to heavy weight. With at least 2 people or using a trolley for assistance. Move the machine slowly, carefully and never be inclined over 45°.
2.2.17 This appliance is equipped with a cord having a grounding wire with a grounding plug, the plug must be plugged into an outlet that is properly installed and grounded.

2.3 Grounding installation
This appliance is classified as protection class I appliance and must be connected to a protective ground. Grounding reduces the risk of electric shock by providing an escape wire for the electric current. This appliance is equipped with a cord having a grounding wire with a grounding plug. The plug must be plugged into an outlet that is properly installed and grounded.

3. [bookmark: _Hlk63171826]PRODUCT DESCRIPTION
3.1 Parts of description
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3.2 [image: ]MAIN TECHNICAL PARAMETERS

	Model
	Voltage
	Power 
	N.W./G.W.
	PACKING SIZE

	SD75SF
	220-240V~
50/60Hz
115V~ 60Hz
	400W
	30.9/40.7 kgs
	58X52X105cm



4. INTRODUCTION
4.1 Preparation for first use
4.1.1 Check to make sure the appliance is undamaged. In case of any damage, contact your supplier immediately and do NOT use the appliance.
4.1.2 Remove all the packing material and protection film (if applicable). Keep the packaging for future storage.
4.1.3 Clean the appliance, see: 4.6 Cleaning.
4.1.4 Place the appliance on a level and steady surface, unless mentioned otherwise.
4.1.5 Make sure there is enough clearance around the appliance for ventilation purposes.
4.1.6 Position the appliance in such a way that the plug is accessible at all times.
4.1.7 The machine must be used only by trained staff with perfect knowledge of the safety standards contained in this manual.
4.1.8 If staff turnover is necessary, provide training beforehand.
4.1.9 Make sure the power outlet ratings correspond to the specifications printed on the rating plate.
4.1.10 Make sure that the machine is connected to a grounding system.
4.1.11 Even if safety systems are installed on the machine, prevent approaching moving parts with hands and do not touch the machine with wet or damp hands.
4.1.12 Disconnect the machine’s socket from the electric before carrying out any cleaning or maintenance operations.
4.1.13 Do not clean with high-pressure water jet.
4.1.14 Regularly check the condition of the power cable. Avoid leaving the power cable in regularly check the condition of the power cable. Avoid leaving the power cable in contact with hot or sharp surfaces and do not pull it in order to remove the plug from the power socket. 
4.1.15 It is strongly recommended that the operator contact the after sales center if there is any problem or malfunction occurred. Please do not dismantle the machine or in place of unauthorized parts.
4.2 The manufacturer will be not responsible for following cases:
4.2.1 If the machine is tampered with or safety functions are installed by non-authorized staff.
4.2.2 If the components are replaced by unauthorized parts.
4.2.3 If the instruction in this manual is not carefully followed.
4.2.4 If the machine surfaces are treated with unsuitable substance or solvent.

4.3 Safety devices 
4.3.1 Micro-switch: The micro-switch is equipped with a magnet mechanism. The appliance stops automatically when the upper lid or the outlet lid is opened during operation.
4.3.2 Overcurrent protection switch (Circuit breaker): The switch is designed to protect the electrical circuit from damage caused by excess current as a result of an overload or short circuit. The switch interrupts current flow after a fault is detected.
Note: To reset the switch, press it after the issue is solved. 

4.4  (
Fig 
1
)[image: ]INSTALLATION
4.4.1 Packing and unpacking
The machine is packed in a carton with plywood pallet to guarantee perfect safety during transport.
Handle the carton in compliance with the instructions.
Open the carton and make sure that all components are intact. Keep the carton for any future machine removal.
Lift the machine according to the instructions and place it in its selected setting for installation.
[bookmark: _GoBack](Fig 1) 
4.4.2 Installation area
The selected machine work setting must be sufficiently lit and have an electric power outlet. The workplace must be sufficiently large, perfectly level and dry. The machine should be installed in non-explosive environments. In any case, installation should be carried out by taking into account any applicable industrial safety regulations in force.

4.4.3 Electric connection
DANGER-CAUTION: Electric connection to the power outlet should be operated by skilled personnel. 
Check for the perfect efficiency of the plant grounding system. Make sure that the line voltage (V) and frequency (Hz) correspond to the machine ratings (refer to the machine identification plate and wiring diagram). The machine comes equipped with an 
electric cable with plug. Plug the machine into a main wall switch with differential.

4.5 OPERATION
4.5.1.1 Vegetable prepared, processed suitably for drying.
4.5.1.2 Place the appliance on stable and flat ground. Secure appliance in position by depressing the brake pedal on each castor (Fig 2).
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Fig 2                               Fig 3

4.5.1.3 Open the hinged lid, put and install the basket into appliance.
4.5.1.4 Relieve the drain tube from pipe clip, and leave the water out correctly.
4.5.1.5 Start the machine by pressing the switch “O”.
4.5.1.6 Turning the timer knob on the required working-cycle time length. The machine will automatically stop and end the set cycle.
4.5.1.7 Pressing switch “I” off, open the hinged lid and take out the bracket and vegetable (Fig 3).
4.5.1.8 Vegetable drying finished, unplug the appliance and clean it.
Caution: Do not overload bracket.


4.6 Cleaning
4.6.1 Clean the machine after each use.
4.6.2 Switch off and unplug the machine before cleaning or maintenance and let it cool down completely.
4.6.3 Do not clean the machine with steel wool, strong chemicals, abrasive or toxic agents, as they may damage the surface of the machine and pose a health hazard.
4.6.4 Use clear water during cleaning. Make sure that the electrical parts/connections of the machine do not become wet or damp.
4.6.5 Do not clean the electric components, e. g. switch, button, timer knob etc., with high pressure water jets or extremely hot steam.
4.6.6 Wipe the outside of the machine at least once a month with a soft damp cloth and, if necessary, a little mild detergent. Also make sure to clean the upper lid (incl. the gasket), delivery chute and basins thoroughly after each use. Dry with a soft dry cloth.
4.6.7 Open the hinged lid and take out the bracket. Clean the bracket and salad spinner chamber interior with a suitable brush. Rinse them with clear water afterward.
4.6.8 The machine may only be used again or stored after it is dried completely.

4.7 Storage
4.7.1 Before reassembling, make sure that all parts are dry. Before storing, remove all residues from the appliance (incl. the basins), disconnect it from the supply and clean the appliance and its accessories thoroughly.
4.7.2 Disconnect the appliance from the water supply and waste water outlet hose.
4.7.3 Store the appliance in a dry, protected environment at room temperature and out of the reach of children.
4.7.4 Keep the upper lid open to avoid smell or mold.
4.7.5 To protect the appliance from dust, cover it with a cloth that allows air circulation inside the appliance.












5. [image: ] Circuit diagram 
















6. Exploded view
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	Part Name

	1
	Lid

	2
	Sealing Ring

	3
	Fastener

	4
	Basket

	5
	Rotating Block

	6
	Housing

	7
	Pipe Clamp

	8
	Electrical Box

	9
	Switch

	10
	Knob For Timmer

	11
	Timer

	12
	S/S tube

	13
	Connector

	14
	Drain Tube

	15
	Hose Clamp

	16
	Locating pin

	17
	Shaft

	18
	Flat Key

	19
	Mechanical Seal

	20
	Bearing

	21
	Circlip

	22
	Motor Fixed plate

	23
	Belt Pulley

	24
	Bottom Plate

	25
	Fixed plate for packing

	26
	3" Castor With Brake

	27
	Motor

	28
	Capacitor

	29
	Motor adjusting block

	30
	Belt

	31
	Power Cord

	32
	Cable Tie

	33
	Overcurrent Protection

	34
	Fixed Shaft For Fastener
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