[bookmark: _Hlk148705829]HTD-20L Tilting Head Removable Bowl Spiral Mixer 20L

Powerful motor, heavy duty
Lowe noise reliable, durable and consistent performance
Guard safe switch
Strong caster and supporting feet design
Single Speed Rised Head and Removable Bowl Spiral Mixer
Bowl volume (L): 20
Bowl Size (mm): φ360x210
Max Dry Flour Capacity (Kg): 8
Max Dough Capacity (Kg): 12
Rotation Speed Bowl/hook (R.P.M.): 16/156
Power (KW / A): 1.5 / 10
G.W/N.W (Kg): 150/134
Machine Size (mm): 750x400x730
Includes stainless steel hook, beater and whisk attachment
Timer: 0-30 minutes
Supplied with castors
Water to flour ratio is 45%-50%

HTD-30L Tilting Head Removable Bowl Spiral Mixer 30L 
Powerful motor, heavy duty
Lowe noise reliable, durable and consistent performance
Guard safe switch
Strong caster and supporting feet design
Bowl volume (L): 30
Bowl Size (mm): φ380x260
Max Dry Flour Capacity (Kg): 12
Max Dough Capacity (Kg): 18
Rotation Speed Bowl/hook (R.P.M.): 16/156
Power (KW / A): 1.5 / 10
G.W/N.W (Kg): 160/142
Machine Size (mm): 790x430x830
Includes stainless steel hook, beater and whisk attachment
Timer: 0-30 minutes
Supplied with castors
Water to flour ratio is 45%-50%


HTD-40L Tilting Head Removable Bowl Spiral Mixer 40L
Powerful motor, heavy duty
Lowe noise reliable, durable and consistent performance
Guard safe switch
Strong caster and supporting feet design
Bowl volume (L): 40
Bowl Size (mm): φ450x270
Max Dry Flour Capacity (Kg): 16
Max Dough Capacity (Kg): 24
Rotation Speed Bowl/hook (R.P.M.): 16/156
Power (KW / A): 2.2 / 10A
G.W/N.W (Kg): 202/173
Machine Size (mm): 860x480x930
Includes stainless steel hook, beater and whisk attachment
Timer: 0-30 minutes
Supplied with castors
Water to flour ratio is 45%-50%






