
Ⅰ.Specification
1). Item No.:
     E500C2

2). Power Rate:      5000W

3). Voltage:

380-400V～3N 
Ⅱ. Importance

Please read carefully the following instructions before using the induction cooker.
1). Do not plug with wet hands in order to avoid getting electric shock.

2). Do not plug into a socket where several other appliances are plugged in.

3). Do not use if the power cord is damaged or the plug does not fit the socket safely.

4). Do not open the cooker to replace spare parts by yourself.

5). Do not use the cooker closed to flame or wet places.

6). Do not use where children can easily touch the cooker, or allow children to use the cooker by themselves.

7). Do not place on unstable surfaces.

8). Do not move the cooker together with a pot.

9). Do not heat a pot empty or overheat to avoid dry boiling.

10). Do not place metallic objects such as knives, forks, spoons, lids, cans, and aluminum foils on the top plate.

11). Use the unit with sufficient space around it. Keep the front side and either right or left side of the unit clear.

12). Do not use the unit on carpet or tablecloth (vinyl) or any other low-heat-resistant article.

13). Do not place a sheet of paper between the pot or the pan and the unit. The paper may get burnt.

14). If the surface is cracked, switch off to avoid the possibility of electric shock and then take to the service

center immediately.

15). Do not block air intake or exhaust vent.

16). Do not touch the top plate right after removing the pot or the pan, as the top plate will still be very hot.

17). Do not place the unite near to the objects which are affected by magnet, such as: radios, televisions, automatic-banking cards and cassette tapes.

18). The power cord must be replaced by qualified technicians.
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 CAUTION: Hot surface. 

20) This appliance is not intended for use by persons (including children) with reduced physical, sensory or mental capabilities, or lack of experience and knowledge, unless they have been given supervision or  instruction concerning use of the appliance by a person responsible for their safety.

21) The temperature of accessible surfaces may be high when the appliance is operating.
22) Aluminium foil and plastic vessels not placed on hot surfaces.
23) the glass‑ceramic surfaces are not to be used for storage.

24) metallic objects such as kitchen utensils, cutlery etc. shall not be placed on the hob surface within the cooking zones since they could get hot;

25) take care when operating the appliance, as rings, watches and similar objects worn by the user could get hot when in close proximity to the hob surface

26) only use vessels of the type and size recommended.

27) After use, switch the hob element off by means of its control. Do not rely on the pan detector.

28) appliance not to be cleaned with water jet;

29) any repairs shall be carried out only by persons trained or recommended by the manufacturer.

30) care be taken to ensure that the splashback and surrounding area free of metallic surfaces
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non-ionizing electromagnetic radiation

32) Appliance is not intended to be operated by means of an external timer or separate remote-control system.
Warning: Children should be supervised to ensure that they do not play with the appliance.   

Ⅲ.How to Use
1). After the power cord is wired, the knob indicator lights up green, indicating that the induction cooker is powered on.

2). Select and twist the knob to the 1st gear, the knob indicator lights up red, indicating that the induction cooker is working, and a prompt sound is issued.

3). The induction cooker has a total of six gears, 0-6 gears

4). If the induction cooker does not detect the pot, it will emit a beeping sound, and then it will automatically shut down after 1 minute.
5). During the working state, the induction cooker will shut off automatically if there is no any operation within 2 hours. 

6). This appliance is liable to get hot during use.

7).The temperature of accessible surfaces may be high when the appliance is operating

Ⅳ.Usable and Non-usable Utensils
1). Usable Pans

Steel or cast iron, enameled iron, stainless steel, Rounded-bottom stainless steel or iron pans/pots .

2). Non-usable Pans

    Heat-resistant glass, ceramic container, copper, aluminum pans/pots, flat-bottom pans/pots.
Ⅴ.How to Clean
1). Unplug and wait until the cooker is cooled down completely. Clean the cooker after using each time.

2). If the pots/pans are used without being cleaned, discoloration or cooked on stains may be caused.

3). Do not use benzine, thinner, scrubbing brush or polishing powder to clean the induction cooker.

4). Wipe using dish washing agent and damp cloth.

5). Use vacuum cleaner to suck up dirt from the air intake and exhaust vent.

6).  Never run water over the unit (Water gets inside may cause malfunction).


